3GPP TS 36.213 V17.1.0 (2022-03)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Radio Access Network;

Evolved Universal Terrestrial Radio Access (E-UTRA);

Physical layer procedures

(Release 17)

** 

The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP.  
The present document has not been subject to any approval process by the 3GPPOrganisational Partners and shall not be implemented.  
This Specification is provided for future development work within 3GPPonly. The Organisational Partners accept no liability for any use of this Specification.  
Specifications and reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organisational Partners' Publications Offices.

Keywords

E-UTRA, radio, layer 1

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles – Sophia Antipolis

Valbonne – France

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword 8

1 Scope 9

2 References 9

3 Symbols and abbreviations 10

3.1 Symbols 10

3.2 Abbreviations 10

4 Synchronization procedures 12

4.1 Cell search 12

4.2 Timing synchronization 12

4.2.1 Radio link monitoring 12

4.2.2 Inter-cell synchronization 12

4.2.3 Transmission timing adjustments 12

4.3 Timing for Secondary Cell Activation / Deactivation 14

5 Power control 15

5.1 Uplink power control 15

5.1.1 Physical uplink shared channel 16

5.1.1.1 UE behaviour 16

5.1.1.2 Power headroom 31

5.1.2 Physical uplink control channel 34

5.1.2.1 UE behaviour 35

5.1.3 Sounding Reference Symbol (SRS) 40

5.1.3.1 UE behaviour 40

5.1.3.2 Power headroom for Type3 report 43

5.1.4 Power allocation for EUTRA dual connectivity 44

5.1.4.1 Dual connectivity power control Mode 1 44

5.1.4.2 Dual connectivity power control Mode 2 51

5.1.4a Power allocation for dual active protocol stack 56

5.1.5 Power allocation for PUCCH-SCell 56

5.2 Downlink power allocation 57

5.2.1 eNodeB Relative Narrowband TX Power (RNTP) restrictions 60

6 Random access procedure 61

6.1 Physical non-synchronized random access procedure 61

6.1.1 Timing 62

6.2 Random Access Response Grant 63

7 Physical downlink shared channel related procedures 68

7.1 UE procedure for receiving the physical downlink shared channel 70

7.1.1 Single-antenna port scheme 89

7.1.2 Transmit diversity scheme 89

7.1.3 Large delay CDD scheme 90

7.1.4 Closed-loop spatial multiplexing scheme 90

7.1.5 Multi-user MIMO scheme 90

7.1.5A Dual layer scheme 90

7.1.5B Up to 8 layer transmission scheme 90

7.1.6 Resource allocation 90

7.1.6.1 Resource allocation type 0 92

7.1.6.2 Resource allocation type 1 93

7.1.6.3 Resource allocation type 2 94

7.1.6.4 PDSCH starting position 97

7.1.6.4A PDSCH starting position for BL/CE UEs 99

7.1.6.5 Physical Resource Block (PRB) bundling 99

7.1.7 Modulation order and transport block size determination 101

7.1.7.1 Modulation order and redundancy version determination 104

7.1.7.2 Transport block size determination 110

7.1.7.2.1 Transport blocks not mapped to two or more layer spatial multiplexing 115

7.1.7.2.2 Transport blocks mapped to two-layer spatial multiplexing 124

7.1.7.2.3 Transport blocks mapped for DCI Format 1C and DCI Format 6-2 124

7.1.7.2.4 Transport blocks mapped to three-layer spatial multiplexing 125

7.1.7.2.5 Transport blocks mapped to four-layer spatial multiplexing 125

7.1.7.2.6 Transport blocks mapped for BL/CE UEs configured with CEModeB and PDSCH bandwidth up to 1.4MHz 126

7.1.7.2.7 Transport blocks mapped for BL/CE UEs *SystemInformationBlockType1-BR* 127

7.1.7.2.8 Transport blocks mapped for UEs configured with *ce-pdsch-maxBandwidth-config* value of 5 MHz or with *pdsch-MaxBandwidth-SC-MTCH* value of 24 PRBs 127

7.1.7.3 Redundancy Version determination for Format 1C 127

7.1.8 Storing soft channel bits 128

7.1.9 PDSCH resource mapping parameters 128

7.1.10 Antenna ports quasi co-location for PDSCH 130

7.1.11 PDSCH subframe assignment for BL/CE UE 131

7.2 UE procedure for reporting Channel State Information (CSI) 133

7.2.1 Aperiodic CSI Reporting using PUSCH 143

7.2.2 Periodic CSI Reporting using PUCCH 169

7.2.3 Channel Quality Indicator (CQI) definition 210

7.2.4 Precoding Matrix Indicator (PMI) definition 224

7.2.5 Channel-State Information – Reference Signal (CSI-RS) definition 252

7.2.6 Channel-State Information – Interference Measurement (CSI-IM) Resource definition 254

7.2.7 Zero Power CSI-RS Resource definition 254

7.2.8 CSI-RS Activation / Deactivation 254

7.3 UE procedure for reporting HARQ-ACK 255

7.3.1 FDD HARQ-ACK reporting procedure 259

7.3.2 TDD HARQ-ACK reporting procedure 264

7.3.2.1 TDD HARQ-ACK reporting procedure for same UL/DL configuration 265

7.3.2.2 TDD HARQ-ACK reporting procedure for different UL/DL configurations 280

7.3.3 FDD-TDD HARQ-ACK reporting procedure for primary cell frame structure type 1 287

7.3.4 FDD-TDD HARQ-ACK reporting procedure for primary cell frame structure type 2 289

8 Physical uplink shared channel related procedures 291

8.0 UE procedure for transmitting the physical uplink shared channel 292

8.0.1 Single-antenna port scheme 319

8.0.2 Closed-loop spatial multiplexing scheme 319

8.1 Resource allocation for PDCCH/EPDCCH/SPDCCH with uplink DCI format 320

8.1.1 Uplink resource allocation type 0 320

8.1.2 Uplink resource allocation type 1 321

8.1.3 Uplink resource allocation type 2 321

8.1.4 Uplink resource allocation type 3 322

8.1.5 Uplink resource allocation type 4 323

8.1.5.1 UL Resource Block Groups 323

8.1.6 Uplink resource allocation type 5 324

8.2 UE sounding procedure 326

8.3 UE HARQ-ACK procedure 338

8.3A Autonomous uplink feedback procedure 340

8.4 UE PUSCH hopping procedure 340

8.4.1 Type 1 PUSCH hopping 341

8.4.2 Type 2 PUSCH hopping 341

8.5 UE Reference Symbol (RS) procedure 342

8.6 Modulation order, redundancy version and transport block size determination 343

8.6.1 Modulation order and redundancy version determination 343

8.6.2 Transport block size determination 351

8.6.3 Control information MCS offset determination 358

8.7 UE transmit antenna selection 362

8.8 Transmission timing adjustments 362

9 Physical downlink control channel procedures 362

9.1 UE procedure for determining physical downlink control channel assignment 363

9.1.1 PDCCH assignment procedure 363

9.1.2 PHICH assignment procedure 367

9.1.3 Control Format Indicator (CFI) assignment procedure 370

9.1.4 EPDCCH assignment procedure 371

9.1.4.1 EPDCCH starting position 378

9.1.4.2 Antenna ports quasi co-location for EPDCCH 378

9.1.4.3 Resource mapping parameters for EPDCCH 379

9.1.4.4 PRB-pair indication for EPDCCH 379

9.1.5 MPDCCH assignment procedure 380

9.1.5.1 MPDCCH starting position 388

9.1.5.2 Antenna ports quasi co-location for MPDCCH 388

9.1.5.3 Preconfigured Uplink Resource ACK/fallback procedure 388

9.1.6 SPDCCH assignment procedure 388

9.1.6.1 Resource mapping parameters for SPDCCH 390

9.1.6.2 PRB-pair indication for SPDCCH 390

9.1.6.3 Physical Resource Block (PRB) bundling for DMRS-based SPDCCH 391

9.1.6.4 Antenna ports quasi co-location for DMRS-based SPDCCH 391

9.2 PDCCH/EPDCCH/MPDCCH/SPDCCH validation for semi-persistent scheduling 392

9.2A PDCCH/EPDCCH validation for autonomous uplink transmissions 394

9.3 PDCCH/EPDCCH/MPDCCH/SPDCCH control information procedure 395

10 Physical uplink control channel procedures 396

10.1 UE procedure for determining physical uplink control channel assignment 397

10.1.1 PUCCH format information 402

10.1.2 FDD HARQ-ACK feedback procedures 409

10.1.2.1 FDD HARQ-ACK procedure for one configured serving cell 409

10.1.2.2 FDD HARQ-ACK procedures for more than one configured serving cell 413

10.1.2.2.1 PUCCH format 1b with channel selection HARQ-ACK procedure 413

10.1.2.2.2 PUCCH format 3 HARQ-ACK procedure 416

10.1.2.2.3 PUCCH format 4 HARQ-ACK procedure 418

10.1.2.2.4 PUCCH format 5 HARQ-ACK procedure 421

10.1.3 TDD HARQ-ACK feedback procedures 422

10.1.3.1 TDD HARQ-ACK procedure for one configured serving cell 424

10.1.3.2 TDD HARQ-ACK procedure for more than one configured serving cell 438

10.1.3.2.1 PUCCH format 1b with channel selection HARQ-ACK procedure 438

10.1.3.2.2 PUCCH format 3 HARQ-ACK procedure 454

10.1.3.2.3 PUCCH format 4 HARQ-ACK procedure 462

10.1.3.2.4 PUCCH format 5 HARQ-ACK procedure 478

10.1.3A FDD-TDD HARQ-ACK feedback procedures for primary cell frame structure type 2 478

10.1.4 HARQ-ACK Repetition procedure 480

10.1.5 Scheduling Request (SR) procedure 481

10.2 Uplink HARQ-ACK timing 483

11 Physical Multicast Channel (PMCH) related procedures 490

11.1 UE procedure for receiving the PMCH 490

11.2 UE procedure for receiving MCCH and system information change notification 493

12 Assumptions independent of physical channel 493

13 Uplink/Downlink configuration determination procedure for Frame Structure Type 2 494

13.1 UE procedure for determining eIMTA-uplink/downlink configuration 495

13A Subframe configuration for Frame Structure Type 3 496

14 UE procedures related to Sidelink 499

14.1 Physical Sidelink Shared Channel related procedures 500

14.1.1 UE procedure for transmitting the PSSCH 500

14.1.1.1 UE procedure for determining subframes for transmitting PSSCH for sidelink transmission mode 1 502

14.1.1.1.1 Determination of subframe indicator bitmap 502

14.1.1.2 UE procedure for determining resource blocks for transmitting PSSCH for sidelink transmission mode 1 505

14.1.1.2.1 PSSCH resource allocation for sidelink transmission mode 1 505

14.1.1.2.2 PSSCH frequency hopping for sidelink transmission mode 1 506

14.1.1.3 UE procedure for determining subframes for transmitting PSSCH for sidelink transmission mode 2 506

14.1.1.4 UE procedure for determining resource blocks for transmitting PSSCH for sidelink transmission mode 2 507

14.1.1.4A UE procedure for determining subframes and resource blocks for transmitting PSSCH for sidelink transmission mode 3 507

14.1.1.4B UE procedure for determining subframes and resource blocks for transmitting PSSCH and reserving resources for sidelink transmission mode 4 508

14.1.1.4C UE procedure for determining subframes and resource blocks for PSSCH transmission associated with an SCI format 1 508

14.1.1.5 UE procedure for PSSCH power control 509

14.1.1.6 UE procedure for determining the subset of resources to be reported to higher layers in PSSCH resource selection in sidelink transmission mode 4 and in sensing measurement in sidelink transmission mode 3 511

14.1.1.7 Conditions for selecting resources when the number of HARQ transmissions is two in sidelink transmission mode 4 514

14.1.2 UE procedure for receiving the PSSCH 514

14.1.3 UE procedure for determining resource block pool and subframe pool for sidelink transmission mode 2 515

14.1.5 UE procedure for determining resource block pool and subframe pool for sidelink transmission mode 3 and 4 516

14.2 Physical Sidelink Control Channel related procedures 517

14.2.1 UE procedure for transmitting the PSCCH 517

14.2.1.1 UE procedure for determining subframes and resource blocks for transmitting PSCCH for sidelink transmission mode 1 520

14.2.1.2 UE procedure for determining subframes and resource blocks for transmitting PSCCH for sidelink transmission mode 2 520

14.2.1.3 UE procedure for PSCCH power control 520

14.2.2 UE procedure for receiving the PSCCH 522

14.2.3 UE procedure for determining resource block pool and subframe pool for PSCCH 522

14.2.4 UE procedure for determining resource block pool for PSCCH in sidelink transmission mode 3 and 4 523

15 Void 526

16 UE Procedures related to narrowband IoT 526

16.1 Synchronization procedures 527

16.1.1 Cell search 527

16.1.2 Timing synchronization 527

16.2 Power control 527

16.2.1 Uplink power control 527

16.2.1.1 Narrowband physical uplink shared channel 528

16.2.1.1.1 UE behaviour 528

16.2.1.1.2 Power headroom 529

16.2.1.2 SR 529

16.2.1.2.1 UE behaviour 529

16.2.2 Downlink power allocation 529

16.3 Random access procedure 530

16.3.1 Physical non-synchronized random access procedure 530

16.3.2 Timing 531

16.3.3 Narrowband random access response grant 532

16.4 Narrowband physical downlink shared channel related procedures 533

16.4.1 UE procedure for receiving the narrowband physical downlink shared channel 534

16.4.1.1 Single-antenna port scheme 538

16.4.1.2 Transmit diversity scheme 538

16.4.1.3 Resource allocation 538

16.4.1.4 NPDSCH starting position 541

16.4.1.5 Modulation order and transport block size determination 542

16.4.1.5.1 Transport blocks not mapped for *SystemInformationBlockType1-NB* 543

16.4.1.5.2 Transport blocks mapped for *SystemInformationBlockType1-NB* 543

16.4.2 UE procedure for reporting ACK/NACK 544

16.5 Narrowband physical uplink shared channel related procedures 545

16.5.1 UE procedure for transmitting format 1 narrowband physical uplink shared channel 546

16.5.1.1 Resource allocation 548

16.5.1.2 Modulation order, redundancy version and transport block size determination 550

16.5.2 UE procedure for NPUSCH retransmission 552

16.5.3 UE procedure for transmitting SR 552

16.6 Narrowband physical downlink control channel related procedures 552

16.6.1 NPDCCH starting position 558

16.6.2 NPDCCH control information procedure 558

16.6.3 NPDCCH validation for semi-persistent scheduling 558

16.6.4 Preconfigured uplink resource ACK/fallback procedure 559

16.7 Assumptions independent of physical channel related to narrowband IoT 559

16.8 UE procedure for acquiring cell-specific reference signal sequence and raster offset 559

16.9 UE procedure for receiving narrowband wake up signal 560

17 Wake-up signal related procedures for BL/CE UE 561

Annex A (informative): Change history 562